***16 BIT SUBTRACTION***

***PROGRAM***

LHLD 2500

XCHG

LHLD 2502

MOV A,E

SUB L

MOV L,A

MOV A,D


ADC H

MOV H,A

SHLD 2504

HLT

***OUTPUT SCREENSHOT***

******