***8 BIT SWAP TWO NUMBERS***

***PROGRAM***

LDA 2500

MOV B,A

LDA 2501


STA 2500

MOV A,B

STA 2501

HLT

***OUTPUT SCREENSHOT***

******