***8 BIT ADDITION***

***PROGRAM***

LDA 8500

MOV BA


LDA 8501

ADD B

STA 8502

HLT

***OUTPUT SCREENSHOT***

******