***8 BIT SUBTRACTION***

***PROGRAM***

LDA 9001

MOV B,A


LDA 9000

SUB B

STA 9002

HLT

***OUTPUT SCREENSHOT***

******